Forklift cotton clip, flat grip clip, waste paper bag clip
Factory direct sales can customize various models
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	Rotary soft-clamp

	model
	carrying capacity @
load center
(kg@mm)
	Installation Class
ISO
	Shoulder range of motion
ITI
(mm)
	brachium L
(mm)
	Arm height
C
(mm)
	Arm thickness
T
(mm)
	width
B
(mm)
	altitude
H
(mm)
	Vertical center of gravity
VCG
(mm)
	Loss of load capacity
ET
(mm)
	Horizontal center of gravity
HCG
(mm)
	conduct oneself with dignity
(kg)

	BCR-20D-01B
	1900@500
	II
	450-1730
	991
	415
	70
	1040
	775
	335
	221
	300
	640

	BCR-20D-01C
	1900@500
	III
	450-1730
	991
	415
	70
	1040
	775
	335
	221
	300
	640

	BCR-20D-02B
	1900@500
	II
	440-1730
	1194
	415
	70
	1040
	775
	335
	221
	368
	683

	BCR-20D-02C
	1900@500
	III
	440-1730
	1194
	415
	70
	1040
	775
	335
	221
	368
	683

	BCR-30D-01B
	2700@500
	II
	550-1900
	991
	460
	75
	1015
	775
	335
	236
	328
	772

	BCR-30D-01C
	2700@500
	III
	550-1900
	991
	460
	75
	1015
	775
	335
	279
	366
	788

	BCR-30D-02B
	2700@500
	II
	550-1900
	1194
	460
	75
	1015
	775
	335
	236
	396
	835

	BCR-30D-02C
	2700@500
	III
	560-1905
	1194
	460
	75
	1015
	775
	335
	279
	432
	854
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	Enhanced soft encapsulation

	model
	carrying capacity @
(kg@mm)
	Installation Class
ISO
	Shoulder range of motion
ITI
(mm)
	brachium L
(mm)
	Arm height
C
(mm)
	Arm thickness
T
(mm)
	width
B
(mm)
	altitude
H
(mm)
	Vertical center of gravity
VCG
(mm)
	Loss of load capacity
ET
(mm)
	Horizontal center of gravity
HCG
(mm)
	conduct oneself with dignity
(kg)

	BCS-30G-01B
	3000@500
	II
	460-2330
	460
	1200
	75
	1680
	740
	250
	150
	300
	750

	BCS-30G-01C
	3000@500
	III
	460-2330
	460
	1200
	75
	1680
	740
	250
	150
	300
	750

	BCS-30G-02B
	3000@500
	II
	460-2330
	460
	1000
	75
	1680
	740
	250
	150
	300
	730

	BCS-30G-02C
	3000@500
	III
	460-2330
	460
	1000
	75
	1680
	740
	250
	150
	300
	730

	BCS-30G-03B
	3000@500
	II
	585-2000
	460
	1200
	75
	1265
	740
	250
	150
	345
	625

	BCS-30G-03C
	3000@500
	III
	585-2000
	460
	1200
	75
	1265
	740
	250
	150
	345
	625

	BCS-30G-04B
	2800@500
	II
	815-2230
	460
	1200
	75
	1330
	740
	250
	150
	345
	730

	BCS-30G-04C
	2800@500
	III
	815-2230
	460
	1200
	75
	1330
	740
	250
	150
	345
	730

	BCS-30G-05B
	3000@500
	II
	520-1870
	460
	1200
	75
	1130
	740
	250
	150
	345
	620

	BCS-30G-05C
	3000@500
	III
	520-1870
	460
	1200
	75
	1130
	740
	250
	150
	345
	620
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	Lateral-shifting soft-clamping device

	model
	carrying capacity @
load center
(kg@mm)
	Installation Class
ISO
	Shoulder range of motion
IT1
(mm)
	brachium L
(mm)
	Arm height
C
(mm)
	Arm thickness
T
(mm)
	width
B
(mm)
	altitude
H
(mm)
	Vertical center of gravity
VCG
(mm)
	Loss of load capacity
ET
(mm)
	Horizontal center of gravity
HCG
(mm)
	conduct oneself with dignity
(kg)

	BCS-20D-01B
	1900@500
	II
	450-1730
	991
	415
	70
	1040
	665
	220
	127
	315
	422

	BCS-20D-01C
	1900@500
	III
	450-1730
	991
	415
	70
	1040
	665
	220
	127
	315
	422

	BCS-20D-02B
	1900@500
	II
	450-1730
	1194
	415
	70
	1040
	665
	220
	127
	401
	465

	BCS-20D-02C
	1900@500
	III
	450-1730
	1194
	415
	70
	1040
	665
	220
	127
	401
	465

	BCS-20D-03B
	1900@500
	II
	455-1735
	685
	415
	70
	1040
	665
	220
	127
	203
	350

	BCS-20D-04B
	1900@500
	II
	455-1735
	785
	415
	70
	1040
	665
	220
	127
	239
	377

	BCS-20D-05B
	1900@500
	II
	450-1730
	915
	415
	70
	1040
	665
	220
	127
	307
	418

	BCS-30D-01B
	2700@500
	II
	550-1900
	991
	460
	75
	1015
	730
	255
	142
	315
	556

	BCS-30D-01C
	2700@500
	III
	550-1900
	991
	460
	75
	1015
	730
	255
	150
	312
	579

	BCS-30D-02B
	2700@500
	II
	550-1900
	1194
	460
	75
	1015
	730
	255
	142
	396
	624

	BCS-30D-02C
	2700@500
	III
	550-1900
	1194
	460
	75
	1015
	730
	255
	150
	391
	640

	BCS-30D-03C
	2700@500
	III
	490-2300
	990
	460
	75
	1600
	730
	255
	150
	240
	710

	BCS-30D-04C
	2200@500
	III
	490-2300
	1194
	460
	75
	1600
	730
	255
	150
	240
	730







Note:				
1. The actual carrying capacity of the forklift and accessories obtained from the forklift manufacturer. 										
2. Forklifts require two additional sets of oil circuits. 									
3. Arm thickness "T" refers to the spatial dimension required for actual operation, which is different from the thickness of the actual arm plate. 									
[bookmark: _GoBack]4. The above types are standard types. If there are special requirements, please contact the sales personnel. 					

*Homsun Machinery Equipment Co., Ltd is a professional manufacture specializing in the R &D and producing of electric scissor lift , electric forklift, mobile yard ramp and motorised pallet truck high-quality hardware accessories. Established in 2016, we have over ten years of experience in the industry, dedicated to providing comprehensive solutions of carrying and lifting for all different industries.

*We are the source manufacturer and can also customize various types of forklifts according to customer needs. 

*If needed, you can consult customer service.

Official website:https://www.homsunlift.com
WhatsApp/Wechat ID:+8613680275183
Email:sandy519@foxmail.com
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