

Special oil bucket clamp for clamp type forklift, oil bucket handling and stacking fixture, bucket holder technical parameters
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	model
	unit
	DG10
	DG20
	DG30
	DG40
	DG45
	DG50

	type
	/
	Single barrel
	Double Barrel
	Single barrel
	Single barrel
	Double Bucket
	Single barrel

	nominal load  capacity
	Kg
	450
	900
	450
	450
	900
	300

	Suitable for oil drum specifications
	/
	55 gallons (φ572 × 900)
	30 gallons (450 × 500) or 55 gallons (φ572 × 900)

	Gantry fork mouth dimensions (length × width)
	mm
	140×55
	178×55
	140×55
	178×55
	178×55
	138×30

	Slot spacing
	mm
	560
	660
	560
	520
	650
	521/616

	net weight
	Kg
	55
	90
	52
	56
	88
	20
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	model
	unit
	DG400
	DG800

	type
	/
	Single barrel
	Double Bucket

	load
	Kg
	400
	800

	net weight
	Kg
	57
	81.7

	Single-shaft sleeve dimensions
	mm
	160*70
	160*70

	Crane sleeve length
	mm
	755
	755

	External dimensions
	mm
	1440*640*590
	1440*1240*590

	Outer width of the fork sleeve
	mm
	640
	735




*Homsun Machinery Equipment Co., Ltd is a professional manufacture specializing in the R &D and producing of electric scissor lift , electric forklift, mobile yard ramp and electric pallet jack  high-quality hardware accessories. Established in 2016, we have over ten years of experience in the industry, dedicated to providing comprehensive solutions of carrying and lifting for all different industries.

*We are the source manufacturer and can also customize various types of forklifts according to customer needs. 

*If needed, you can consult customer service.

Official website:https://www.homsunlift.com
WhatsApp/Wechat ID:+8613680275183
Email:sandy519@foxmail.com

Related product recommendations：
Forklift clamp type oil drum clamp
Oil Drum Flipper
Electric Drum Dumping Truck
Oil drum lifting vehicle
Oil Drum Truck
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