Technical Parameters of High end reinforced tipping waste paper clip forklift accessories

Factory direct sales can customize various models

	model
	Installation Class
	Number of rake claws
	Rake claw width (RW)
MM
	Beam width A
mm
	Arm reach range
mm
	weight capacity
kg
	Suitable for forklifts
t

	CYQ2A30
	Ⅲ
	7
	1300
	1500
	0-2350
	3000
	3-3.5


Remarks:
The forklift is required to be fitted with 2 sets of oil circuits.
Fork tines are not included; they can be fitted as required.
Custom sizes are available.
Application:
Mainly used for handling, clamping and tilting operations of waste paper, grass, iron scraps, round logs and other materials. A bucket can also be installed for clamping and handling bulk goods. Simple and fast operation improves work efficiency, saves energy, maximizes the forklift’s performance and reduces labour costs.
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Structural line diagram

*****************************************************************************
The meaning of accessory installation level
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	Installation level
	Ⅱ
	Ⅲ
	Ⅳ
	Ⅴ

	Rated lifting capacity of forklift (kg)
	1000-2500
	2501-4999
	5000-8000
	8001-10999


*Homsun Machinery Equipment Co., Ltd is a professional manufacture specializing in the R &D and producing of electric scissor lift , electric forklift, mobile yard ramp and motorised pallet truck high-quality hardware accessories. Established in 2016, we have over ten years of experience in the industry, dedicated to providing comprehensive solutions of carrying and lifting for all different industries.

*We are the source manufacturer and can also customize various types of forklifts according to customer needs. 

*If needed, you can consult customer service.
Official website:https://www.homsunlift.com

WhatsApp/Wechat ID:+8613680275183

Email:sandy519@foxmail.com
Related product recommendations：

Oil Drum Dumping
Forklift Push-Pull
Small tonnage rack
Side shifter belt
